Hobo RH/T sensor located 1 meter above ground

Sensor name: SG\_North\_Hilltop\_1 meter

S 20º57.205

W 70º01.168

Alt: 684 m

Deployed on March 25 at 9 am

Collects data every 30 min (1.2 years)

Battery good